This Amend a DOC is certified with CT19.1, but testing here used CT21 to be more up to date.

Some testing notes:
- The "Interactive Test Sequencer - QoS Object Behavior Test" used CT20 instead of CT21 (because CT21 triggered some errors).
- The "errors" in the logs are OK since this HMI product has a GUI to set speed/duplex and is purposely not allowed to be set via CIP:

*** The DUT does not support manual setting speed and duplex via CIP interface but forced speed 100Mbs and full duplex is required for a DLR capable device. [Vol 2 section 9-5.6]. This error can be waived if the DUT supports other means to set speed/duplex.

Amend a DOC File Artifacts:
- .log files for two DUTs in the family in both DHCP and static IP configurations.
- Results of the CT software's Interactive Tests.
- EDS files.
- EZEDS.exe log files for each EDS file.
- NMAP result files.
- User Manual URL: https://literature.rockwellautomation.com/idc/groups/literature/documents/um/2711p-um008_-en-p.pdf